|  |  |
| --- | --- |
| **Product Description** |  |
|  |  |
| **Heavy Duty Toggle Clamp Flat** **Base Slotted Arm Size 300daN** |
| **Key Features** |  |
|  |  |
| **Overall Height:** | **122mm** |
| **Underarm Height:** | **27mm** |
| **Arm Length:** | **45mm** |
| **Holding Force:** | **300daN** |
|  |  |
| **Other Features** |  |
|  |  |
| **Arm Opens:** | **134°** |
| **Handle Opens:** | **210°** |
| **Weight:** | **0.31Kg** |
|  |  |
|  |  |
| **Material** |  |
| **Toggle Clamp:** | **Cast Iron** |
| **Spindle:** | **Zinc Plated Mild Steel** |
| **Handle:** | **uPVC** |
| **Flanged Washers:** | **Zinc Plated Mild Steel** |
|  |  |
|  | **Whats In The Bag?** |
|  |  |
| **Toggle Clamp:** | **GH-70320-B** |
| **Spindle:** | **SA-065010** |
| **2x Flanged Washers** | **FW-142** |
|  |  |



